! /INPUT,VABS_APDL_Graphic/EPSGen,mac

! General method to save a picture from the ANSYS screen
! (1) use the following command to generate a PostScript (.eps) file 
! Use Inkscape to import .eps and .png file
! Use Adobe pro to import .eps and export .pdf


!==============================================================
/SHOW,PSCR  
!PSCR,HIRES,0
PSCR,HIRES,1          ! high resolution
/DEVICE,VECTOR,0
/GFILE,1200,
!*  
PSCR,PAPER,A,PORT  
! PSCR,PAPER,A,Landscape
PSCR,COLOR,2
PSCR,TIFF,0 
PSCR,LWID,1            ! Line width factor, use skinny lines
!*  
/CMAP,_TEMPCMAP_,CMP,,SAVE  
!	/RGB,INDEX,100,100,100,0
!	/RGB,INDEX,0,0,0,15 
/REPLOT 
/CMAP,_TEMPCMAP_,CMP
/DELETE,_TEMPCMAP_,CMP  
/SHOW,CLOSE 
/DEVICE,VECTOR,0
!==============================================================